1. 50Hz or higher.
2. Given 100,000,000Hz=2^x\*200Hz, x is equal to 18.9. So at **count[18]** we use the minimum to counter width to give each display digit at least 50Hz.